{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":100,"n_cols":4,"rows_kept":100,"merged":[[0,1,0,3],[50,1,52,1],[53,1,56,1],[57,1,59,1],[80,1,82,1],[83,1,86,1],[87,1,89,1]],"flags":["formulas_cached_only"]}
[null,"风火轮说明书"]
[null,"Addr","A001-A512","512地址设置"]
[]
[null,"CHnd","23CH","23通道设置"]
[null,null,"16CH","16通道设置"]
[]
[null,"SLnd","Auto","主机自走模式"]
[null,null,"Soun","主机声控模式"]
[null,null,"SL 1","控台模式"]
[null,null,"SL 2","副机模式"]
[]
[null,"SHnd","SH 0","效果0（推荐）"]
[null,null,"SH 1","效果1"]
[null,null,"SH 2","效果2"]
[null,null,"SH 3","效果3"]
[]
[]
[null,"SEnS","0-99","声控灵敏度体调节"]
[]
[null,"bLAnd","bLAc","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Soun","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态"]
[]
[null,"LEd","OFF","5秒后灭屏"]
[null,null,"ON","屏幕一直开启"]
[]
[null,"dISP","no","显示反向"]
[null,null,"YES","显示正向"]
[]
[null,"rPAn","no","X电机正转"]
[null,null,"YES","X电机反转"]
[]
[null,"TiL1","no","Y1电机正转"]
[null,null,"YES","Y1电机反转"]
[]
[null,"TiL2","no","Y2电机正转"]
[null,null,"YES","Y2电机反转"]
[]
[null,"REST","YES","系统复位"]
[]
[null,"16通道模式"]
[null,"通道","数据","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","Y1电机运转"]
[null,3,"6-255","Y1电机无极运转"]
[null,4,"0-255","Y2电机运转"]
[null,5,"6-255","Y2电机无极运转"]
[null,6,"0-255","电机速度"]
[null,7,"0-255","总调光"]
[null,8,"0","无频闪"]
[null,null,"1-250","频闪"]
[null,null,"251-255","无频闪"]
[null,9,"0","调光通道作用"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","走灯效果"]
[null,null,"141-255","声孔走灯效果"]
[null,10,"0-15","其他通道作用"]
[null,null,"15-128","自走效果"]
[null,null,"129-255","声控效果"]
[null,11,"0-255","控制9  10的速度及灵敏度"]
[null,12,"0-255","红色1-2总调光"]
[null,13,"0-255","绿色1-2总调光"]
[null,14,"0-255","蓝色1-2总调光"]
[null,15,"0-255","白色1-2总调光"]
[null,16,"250-255","复位"]
[]
[]
[null,"23通道模式"]
[null,"通道","数据","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","X电机微调"]
[null,3,"0-255","Y1电机运转"]
[null,4,"0-255","Y1电机微调"]
[null,5,"6-255","Y1电机无极运转"]
[null,6,"0-255","Y2电机运转"]
[null,7,"0-255","Y2电机微调"]
[null,8,"6-255","Y2电机无极运转"]
[null,9,"0-255","电机速度"]
[null,10,"0-255","总调光"]
[null,11,"0","无频闪"]
[null,null,"1-250","频闪"]
[null,null,"251-255","无频闪"]
[null,12,"0","调光通道作用"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","走灯效果"]
[null,null,"141-255","声孔走灯效果"]
[null,13,"0-15","其他通道作用"]
[null,null,"15-128","自走效果"]
[null,null,"129-255","声控效果"]
[null,14,"0-255","控制12  13的速度及灵敏度"]
[null,15,"0-255","红色1总调光"]
[null,16,"0-255","绿色1总调光"]
[null,17,"0-255","蓝色1总调光"]
[null,18,"0-255","白色1总调光"]
[null,19,"0-255","红色2总调光"]
[null,20,"0-255","绿色2总调光"]
[null,21,"0-255","蓝色2总调光"]
[null,22,"0-255","白色2总调光"]
[null,23,"250-255","复位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}