{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":92,"n_cols":4,"rows_kept":92,"merged":[[0,1,0,3],[69,1,72,1]],"flags":["formulas_cached_only"]}
[null,"LED摇头蜘蛛灯说明书"]
[]
[null,"d001","001-512","512地址设置"]
[]
[null,"CHxx",13,"13通道设置"]
[null,null,20,"20通道设置"]
[null,null,16,"16通道设置"]
[]
[null,"Mode","DMX","控台模式"]
[null,null,"FAST","快速运行模式"]
[null,null,"SLOW","慢速运行模式"]
[null,null,"SOUN","声控运行模式"]
[]
[null,"SENS","0-99","声控灵敏度体调节"]
[]
[null,"PAN","OFF","X电机正转"]
[null,null,"ON","X电机反转"]
[]
[null,"TiL1","OFF","M1电机正转"]
[null,null,"ON","M1电机反转"]
[]
[null,"TiL2","OFF","M2电机正转"]
[null,null,"ON","M2电机反转"]
[]
[null,"rdoF","rdoF","正向显示"]
[null,null,"rdon","反向显示"]
[]
[null,"CdoF","CdoF","显示不关闭"]
[null,null,"Cdon","显示关闭"]
[]
[null,"Deft ","YES","初始化出厂"]
[]
[null,"REST","YES","系统复位"]
[]
[null,"13通道模式"]
[null,"通道","功能","说明"]
[null,1,"X电机运转","0-255 向上调节正转，向下调节反转"]
[null,2,"X电机速度","0-255 X电机速度调节"]
[null,3,"M1运转","0-255 向上调节正转，向下调节反转"]
[null,4,"M2运转","0-255 向上调节正转，向下调节反转"]
[null,5,"M12电机速度","0-255 M12电机速度调节"]
[null,7,"总调光","0-255 亮度整体调节"]
[null,6,"频闪","0-255频闪调节，由慢到快"]
[null,8,"BAR15调光","0-255 BAR15亮度调节"]
[null,9,"BAR26调光","0-255 BAR26亮度调节"]
[null,10,"BAR37调光","0-255 BAR37亮度调节"]
[null,11,"BAR48调光","0-255 BAR48亮度调节"]
[null,12,"LED效果","LED效果选择"]
[null,13,"LED速度","LED效果运行速度"]
[null,"16通道模式"]
[null,"通道","功能","说明"]
[null,1,"X电机运转","0-255 向上调节正转，向下调节反转"]
[null,2,"X电机速度","0-255 X电机速度调节"]
[null,3,"M1运转","0-255 向上调节正转，向下调节反转"]
[null,4,"M2运转","0-255 向上调节正转，向下调节反转"]
[null,5,"M12电机速度","0-255 M12电机速度调节"]
[null,6,"总调光","0-255 亮度整体调节"]
[null,7,"频闪","0-255频闪调节，由慢到快"]
[null,8,"BAR1调光","0-255 BAR1亮度调节"]
[null,9,"BAR2调光","0-255 BAR2亮度调节"]
[null,10,"BAR3调光","0-255 BAR3亮度调节"]
[null,11,"BAR4调光","0-255 BAR4亮度调节"]
[null,12,"BAR5调光","0-255 BAR5亮度调节"]
[null,13,"BAR6调光","0-255 BAR6亮度调节"]
[null,14,"BAR7调光","0-255 BAR7亮度调节"]
[null,15,"BAR8调光","0-255 BAR8亮度调节"]
[null,16,"系统复位","150-200系统复位"]
[null,"20通道模式"]
[null,"通道","功能","说明"]
[null,"1（内置效果）","0-10","其他通道作用"]
[null,null,"11-120","效果1"]
[null,null,"121-243","效果2"]
[null,null,"245-255","声控效果"]
[null,2,"内置效果速度","内置效果速度调节"]
[null,3,"LED效果","LED效果选择"]
[null,4,"LED速度","LED效果运行速度"]
[null,5,"X电机运转","0-255 向上调节正转，向下调节反转"]
[null,6,"X电机速度","0-255 X电机速度调节"]
[null,7,"M1运转","0-255 向上调节正转，向下调节反转"]
[null,8,"M2运转","0-255 向上调节正转，向下调节反转"]
[null,9,"M12电机速度","0-255 M12电机速度调节"]
[null,10,"总调光","0-255 亮度整体调节"]
[null,11,"频闪","0-255频闪调节，由慢到快"]
[null,12,"BAR1调光","0-255 BAR1亮度调节"]
[null,13,"BAR2调光","0-255 BAR2亮度调节"]
[null,14,"BAR3调光","0-255 BAR3亮度调节"]
[null,15,"BAR4调光","0-255 BAR4亮度调节"]
[null,16,"BAR5调光","0-255 BAR5亮度调节"]
[null,17,"BAR6调光","0-255 BAR6亮度调节"]
[null,18,"BAR7调光","0-255 BAR7亮度调节"]
[null,19,"BAR8调光","0-255 BAR8亮度调节"]
[null,20,"系统复位","150-200系统复位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}