{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":110,"n_cols":4,"rows_kept":110,"merged":[[0,1,0,3],[48,1,51,1],[56,1,61,1],[72,1,75,1],[79,1,88,1],[89,1,94,1]],"flags":["formulas_cached_only"]}
[null,"LED摇头灯说明书-60W"]
[null,"Addr","A001-A512","512地址设置"]
[]
[null,"CHnd","11CH","11通道设置"]
[null,null,"9CH","9通道设置"]
[]
[null,"SLnd","MAST","主机模式"]
[null,null,"SL 1","控台模式"]
[null,null,"SL 2","副机模式"]
[]
[null,"ID","ID00-ID15","ID设置"]
[]
[null,"SHnd","SH 0","效果0（推荐）"]
[null,null,"SH 1","效果1"]
[null,null,"SH 2","效果2"]
[null,null,"SH 3","效果3"]
[]
[null,"Soud","on","声控开启"]
[null,null,"oFF","声控关闭"]
[]
[null,"SEnS","0-99","声控灵敏度体调节"]
[]
[null,"bLAnd","bLAc","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Soun","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态"]
[]
[null,"LEd","OFF","5秒后灭屏"]
[null,null,"ON","屏幕一直开启"]
[]
[null,"dISP","no","显示反向"]
[null,null,"YES","显示正向"]
[]
[null,"rPAN","no","X电机正转"]
[null,null,"YES","X电机反转"]
[]
[null,"rTiL","no","Y电机正转"]
[null,null,"YES","Y电机反转"]
[]
[null,"REST","YES","系统复位"]
[]
[null,"9通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"垂直运转","0-255"]
[null,3,"颜色"]
[null,null,"0-139","选色"]
[null,null,"140-255","自动换色 由慢到快"]
[null,4,"图案"]
[null,null,"0-63","固定图案"]
[null,null,"64-127","图案抖动"]
[null,null,"128-255","自动换图案 由慢到快"]
[null,5,"频闪","0-255"]
[null,6,"调光","0-255"]
[null,7,"水平垂直运转","0-255 "]
[null,8,"自动模式","0-255 向上调节正转，向下调节反转"]
[null,9,"0-10","其他模式作用"]
[null,null,"11-20","ID延时（ID0-ID15）"]
[null,null,"21-100","X电机自动模式"]
[null,null,"101-200","Y电机自动模式"]
[null,null,"201-249","XY电机自动模式"]
[null,null,"复位","250-255（5秒）"]
[]
[null,"11通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"水平微调","0-255"]
[null,3,"垂直运转","0-255"]
[null,4,"垂直微调","0-255"]
[null,5,"颜色"]
[null,null,"0-139","选色"]
[null,null,"140-255","自动换色 由慢到快"]
[null,6,"图案"]
[null,null,"0-63","固定图案"]
[null,null,"64-127","图案抖动"]
[null,null,"128-255","自动换图案 由慢到快"]
[null,7,"频闪","0-255"]
[null,8,"调光","0-255"]
[null,9,"水平垂直运转速度","0-255 "]
[null,10,"自动模式"]
[null,null,"0-59","其他通道作用"]
[null,null,"60-84","自动模式3"]
[null,null,"85-109","自动模式2"]
[null,null,"110-134","自动模式1"]
[null,null,"135-159","自动模式0"]
[null,null,"160-184","声孔模式3"]
[null,null,"185-209","声孔模式2"]
[null,null,"210-234","声孔模式1"]
[null,null,"235-255","声孔模式0"]
[null,11,"0-10","其他模式作用"]
[null,null,"11-20","ID延时（ID0-ID15）"]
[null,null,"21-100","X电机自动模式"]
[null,null,"101-200","Y电机自动模式"]
[null,null,"201-249","XY电机自动模式"]
[null,null,"复位","250-255（5秒）"]
[]
[]
[]
[null,"说明：设置为保持模式时，先拔掉512信号线，等30秒种，"]
[null,"      再关闭电源，系统自动保存最后一次的512信号"]
[null,"      "]
[null,"关于微调：","在A001时候按第四键10秒左右，系统会调出一个菜单"]
[null,null,"H000-255","X电机偏移数据"]
[null,null,"Y000-255","Y电机偏移数据"]
[null,null,"C000-255","色片电机偏移数据"]
[null,null,"G000-255","图岸电机偏移数据"]
[null,null,"DEFR","上面的四个参数出厂初始化"]
[]
[null,null,"再按第四键10秒左右，系统自动保存"]
[null,null,"这步不可少，不然保存不了"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}