{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":177,"n_cols":4,"rows_kept":177,"merged":[[0,1,0,3],[44,1,46,1],[47,1,49,1],[51,1,53,1],[54,1,57,1],[58,1,66,1],[79,1,81,1],[82,1,84,1],[86,1,88,1],[89,1,92,1],[93,1,101,1],[127,1,129,1],[130,1,132,1],[134,1,136,1],[137,1,140,1],[141,1,149,1]],"flags":["formulas_cached_only"]}
[null,"16头幻影灯说明书"]
[null,"DmxSet Address","001-512","512地址设置"]
[]
[null,"Channel    Set","15CH","15通道设置（简单）"]
[null,null,"27CH","27通道设置（推荐 合适做效果）"]
[null,null,"75CH","75通道设置"]
[]
[null,"Mode       Set","Auto","自动模式"]
[null,null,"Soun","声控模式"]
[null,null,"Slve 1","控台模式"]
[null,null,"Slve 2","副机模式"]
[]
[null,"Show      Mode","Show 0","效果0（推荐 包括1 2 3）"]
[null,null,"Show 1","效果1"]
[null,null,"Show 2","效果2"]
[null,null,"Show 3","效果3"]
[]
[]
[null,"Sound     Sense","0-99","声控灵敏度体调节"]
[]
[null,"Nodmx      Set","Blac","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Sound","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态(15通道)"]
[]
[null,"While      Blance","RED","0-255 白平调节"]
[null,null,"Green","0-255 白平调节"]
[null,null,"Blue","0-255 白平调节"]
[null,null,"While","0-255 白平调节"]
[]
[null,"Pan     Inverse","OFF","X电机正转"]
[null,null,"ON","X电机反转"]
[]
[null,"tilt     Inverse","OFF","Y电机正转"]
[null,null,"ON","Y电机反转"]
[]
[null,"Fixture     Rest","YES","系统复位"]
[]
[]
[null,"15通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","Y电机运转"]
[null,3,"0-255","X Y电机速度"]
[null,4,"0-9","无"]
[null,null,"10-127","X电机无及正转"]
[null,null,"128-255","X电机无及反转"]
[null,5,"0-5","无"]
[null,null,"6-127","Y电机无及正转"]
[null,null,"128-255","Y电机无及反转"]
[null,6,"0-255","0-255 亮度整体调节"]
[null,7,"0-9","无"]
[null,null,"9-249","频闪调节，由慢到快"]
[null,null,"250-255","无"]
[null,"8  LED宏功能",0,"无效果"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","自走效果（推荐）"]
[null,null,"140-255","声控效果"]
[null,9,"0-15","无效果"]
[null,null,"16-44","自走效果3"]
[null,null,"45-74","自走效果2"]
[null,null,"75-104","自走效果1"]
[null,null,"105-128","自走效果0（推荐）"]
[null,null,"129-157","声控效果3"]
[null,null,"158-187","声控效果2"]
[null,null,"188-217","声控效果1"]
[null,null,"218-255","声控效果0（推荐）"]
[null,10,"0-255","速度/声控灵敏度"]
[null,11,"0-255","0-255 红色1-15亮度调节"]
[null,12,"0-255","0-255 绿色1-15亮度调节"]
[null,13,"0-255","0-255 蓝色1-15亮度调节"]
[null,14,"0-255","0-255 白色1-15亮度调节"]
[null,15,"150-200","复位"]
[]
[null,"27通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","Y电机运转"]
[null,3,"0-255","X Y电机速度"]
[null,4,"0-9","无"]
[null,null,"10-127","X电机无及正转"]
[null,null,"128-255","X电机无及反转"]
[null,5,"0-5","无"]
[null,null,"6-127","Y电机无及正转"]
[null,null,"128-255","Y电机无及反转"]
[null,6,"0-255","0-255 亮度整体调节"]
[null,7,"0-9","无"]
[null,null,"9-249","频闪调节，由慢到快"]
[null,null,"250-255","无"]
[null,"8  LED宏功能",0,"无效果"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","自走效果（推荐）"]
[null,null,"140-255","声控效果"]
[null,9,"0-15","无效果"]
[null,null,"16-44","自走效果0（推荐）"]
[null,null,"45-74","自走效果1"]
[null,null,"75-104","自走效果2"]
[null,null,"105-128","自走效果3"]
[null,null,"129-157","声控效果0（推荐）"]
[null,null,"158-187","声控效果1"]
[null,null,"188-217","声控效果2"]
[null,null,"218-255","声控效果3"]
[null,10,"0-255","速度/声控灵敏度"]
[null,11,"0-255","0-255 BAR1灯珠亮灭组合  "]
[null,12,"0-255","0-255 BAR2灯珠亮灭组合  "]
[null,13,"0-255","0-255 BAR3灯珠亮灭组合  "]
[null,14,"0-255","0-255 BAR4灯珠亮灭组合  "]
[null,15,"0-255","0-255 BAR5灯珠亮灭组合  "]
[null,16,"0-255","0-255 BAR6灯珠亮灭组合  "]
[null,17,"0-255","0-255 BAR7灯珠亮灭组合  "]
[null,18,"0-255","0-255 BAR8灯珠亮灭组合  "]
[null,19,"0-255","0-255 BAR9灯珠亮灭组合  "]
[null,20,"0-255","0-255 BAR10灯珠亮灭组合  "]
[null,21,"0-255","0-255 BAR11灯珠亮灭组合  "]
[null,22,"0-255","0-255 BAR12灯珠亮灭组合  "]
[null,23,"0-255","0-255 BAR13灯珠亮灭组合  "]
[null,24,"0-255","0-255 BAR14灯珠亮灭组合  "]
[null,25,"0-255","0-255 BAR15灯珠亮灭组合  "]
[null,26,"0-255","0-255 BAR16灯珠亮灭组合  "]
[null,27,"150-200","复位"]
[]
[]
[null,"75通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","Y电机运转"]
[null,3,"0-255","X Y电机速度"]
[null,4,"0-9","无"]
[null,null,"10-127","X电机无及正转"]
[null,null,"128-255","X电机无及反转"]
[null,5,"0-5","无"]
[null,null,"6-127","Y电机无及正转"]
[null,null,"128-255","Y电机无及反转"]
[null,6,"0-255","0-255 亮度整体调节"]
[null,7,"0-9","无"]
[null,null,"9-249","频闪调节，由慢到快"]
[null,null,"250-255","无"]
[null,"8  LED宏功能",0,"无效果"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","自走效果（推荐）"]
[null,null,"140-255","声控效果"]
[null,9,"0-15","无效果"]
[null,null,"16-44","自走效果0（推荐）"]
[null,null,"45-74","自走效果1"]
[null,null,"75-104","自走效果2"]
[null,null,"105-128","自走效果3"]
[null,null,"129-157","声控效果0（推荐）"]
[null,null,"158-187","声控效果1"]
[null,null,"188-217","声控效果2"]
[null,null,"218-255","声控效果3"]
[null,10,"0-255","速度/声控灵敏度"]
[null,11,"0-255","0-255 BAR1红色亮度 "]
[null,12,"0-255","0-255 BAR1绿色亮度 "]
[null,13,"0-255","0-255 BAR1蓝色亮度 "]
[null,14,"0-255","0-255 BAR1白色亮度 "]
[null,15,"0-255","0-255 BAR2红色亮度 "]
[null,16,"0-255","0-255 BAR2绿色亮度 "]
[null,17,"0-255","0-255 BAR2蓝色亮度 "]
[null,18,"0-255","0-255 BAR2白色亮度 "]
[null,19,"0-255","0-255 BAR3红色亮度 "]
[null,20,"0-255","0-255 BAR3绿色亮度 "]
[null,21,"0-255","0-255 BAR3蓝色亮度 "]
[null,22,"0-255","0-255 BAR3白色亮度 "]
[null,23,"0-255","0-255 BAR4红色亮度 "]
[null,24,"0-255","0-255 BAR4绿色亮度 "]
[null,25,"0-255","0-255 BAR4蓝色亮度 "]
[null,26,"0-255","0-255 BAR4白色亮度 "]
[null,27,"0-255","0-255 BAR5红色亮度 "]
[null,28,"0-255","0-255 BAR5绿色亮度 "]
[null,29,"0-255","0-255 BAR5蓝色亮度 "]
[null,30,"0-255","0-255 BAR5白色亮度 "]
[]
[null,71,"0-255","0-255 BAR16红色亮度 "]
[null,72,"0-255","0-255 BAR16绿色亮度 "]
[null,73,"0-255","0-255 BAR16蓝色亮度 "]
[null,74,"0-255","0-255 BAR16白色亮度 "]
[null,75,"150-200","复位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}