{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":111,"n_cols":4,"rows_kept":111,"merged":[[0,1,0,3],[41,1,43,1],[49,1,51,1],[52,1,55,1],[56,1,64,1],[75,1,77,1],[83,1,85,1],[86,1,89,1],[90,1,98,1]],"flags":["formulas_cached_only"]}
[null,"九头光束说明书"]
[null,"DmxSet Address","001-512","512地址设置"]
[]
[null,"Channel    Set","16CH","16通道设置"]
[null,null,"48CH","48通道设置"]
[]
[null,"Mode       Set","Auto","自动模式"]
[null,null,"Soun","声控模式"]
[null,null,"Slve 1","控台模式"]
[null,null,"Slve 2","副机模式"]
[]
[null,"Show      Mode","Show 0","效果0（推荐 包括1 2 3）"]
[null,null,"Show 1","效果1"]
[null,null,"Show 2","效果2"]
[null,null,"Show 3","效果3"]
[]
[]
[null,"Sound     Sense","0-99","声控灵敏度体调节"]
[]
[null,"Nodmx      Set","Blac","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Sound","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态(16通道)"]
[]
[null,"While      Blance","RED","0-255 白平调节"]
[null,null,"Green","0-255 白平调节"]
[null,null,"Blue","0-255 白平调节"]
[null,null,"While","0-255 白平调节"]
[]
[null,"Pan     Inverse","OFF","X电机正转"]
[null,null,"ON","X电机反转"]
[]
[null,"tilt     Inverse","OFF","Y13电机正转"]
[null,null,"ON","Y13电机反转"]
[]
[null,"Fixture     Rest","YES","系统复位"]
[]
[]
[null,"16通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-5","无"]
[null,null,"6-127","X电机无及正转"]
[null,null,"128-255","X电机无及反转"]
[null,3,"0-255","Y1电机运转"]
[null,4,"0-255","Y2电机运转"]
[null,5,"0-255","Y3电机运转"]
[null,6,"0-255","X Y1-3电机速度"]
[null,7,"0-255","0-255 亮度整体调节"]
[null,8,"0-9","无"]
[null,null,"9-249","频闪调节，由慢到快"]
[null,null,"250-255","无"]
[null,"9  LED宏功能",0,"无效果"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","自走效果（推荐）"]
[null,null,"140-255","声控效果"]
[null,10,"0-15","无效果"]
[null,null,"16-44","自走效果0（推荐）"]
[null,null,"45-74","自走效果1"]
[null,null,"75-104","自走效果2"]
[null,null,"105-128","自走效果3"]
[null,null,"129-157","声控效果0（推荐）"]
[null,null,"158-187","声控效果1"]
[null,null,"188-217","声控效果2"]
[null,null,"218-255","声控效果3"]
[null,11,"0-255","速度/声控灵敏度"]
[null,12,"0-255","0-255 红色1-9亮度调节"]
[null,13,"0-255","0-255 绿色1-9亮度调节"]
[null,14,"0-255","0-255 蓝色1-9亮度调节"]
[null,15,"0-255","0-255 白色1-9亮度调节"]
[null,16,"250-255","复位"]
[]
[null,"48通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-5","无"]
[null,null,"6-127","X电机无及正转"]
[null,null,"128-255","X电机无及反转"]
[null,3,"0-255","Y1电机运转"]
[null,4,"0-255","Y2电机运转"]
[null,5,"0-255","Y3电机运转"]
[null,6,"0-255","X Y1-3电机速度"]
[null,7,"0-255","0-255 亮度整体调节"]
[null,8,"0-9","无"]
[null,null,"9-249","频闪调节，由慢到快"]
[null,null,"250-255","无"]
[null,"9  LED宏功能",0,"无效果"]
[null,null,"1-7","渐变效果"]
[null,null,"8-140","自走效果（推荐）"]
[null,null,"140-255","声控效果"]
[null,10,"0-15","无效果"]
[null,null,"16-44","自走效果0（推荐）"]
[null,null,"45-74","自走效果1"]
[null,null,"75-104","自走效果2"]
[null,null,"105-128","自走效果3"]
[null,null,"129-157","声控效果0（推荐）"]
[null,null,"158-187","声控效果1"]
[null,null,"188-217","声控效果2"]
[null,null,"218-255","声控效果3"]
[null,11,"0-255","速度/声控灵敏度"]
[null,12,"0-255","0-255 红色1亮度调节"]
[null,13,"0-255","0-255 绿色1亮度调节"]
[null,14,"0-255","0-255 蓝色1亮度调节"]
[null,15,"0-255","0-255 白色1亮度调节"]
[null,16,"0-255","0-255 红色2亮度调节"]
[null,17,"0-255","0-255 绿色2亮度调节"]
[null,18,"0-255","0-255 蓝色2亮度调节"]
[null,19,"0-255","0-255 白色2亮度调节"]
[]
[]
[null,48,"250-255","复位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}