{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":74,"n_cols":4,"rows_kept":74,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
[null,"LED 4颗调焦说明书"]
[null,"Addr","A001-A512","512地址设置"]
[]
[null,"CHnd","15CH","16通道设置"]
[null,null,"13CH","14通道设置"]
[]
[null,"SLnd","Auto","主机自走模式"]
[null,null,"Soun","主机声控模式"]
[null,null,"SL 1","控台模式"]
[null,null,"SL 2","副机模式"]
[]
[null,"ID","ID00-ID15","ID设置"]
[]
[null,"SHnd","SH 0","效果0（推荐）"]
[null,null,"SH 1","效果1"]
[null,null,"SH 2","效果2"]
[null,null,"SH 3","效果3"]
[]
[]
[null,"SEnS","0-99","声控灵敏度体调节"]
[]
[null,"bLAnd","bLAc","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Soun","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态"]
[]
[null,"LEd","OFF","5秒后灭屏"]
[null,null,"ON","屏幕一直开启"]
[]
[null,"dISP","no","显示反向"]
[null,null,"YES","显示正向"]
[]
[null,"rPAN","no","X电机正转"]
[null,null,"YES","X电机反转"]
[]
[null,"rTiL","no","Y电机正转"]
[null,null,"YES","Y电机反转"]
[]
[null,"REST","YES","系统复位"]
[]
[]
[null,"15通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"水平微调","0-255"]
[null,3,"垂直运转","0-255"]
[null,4,"垂直微调","0-255"]
[null,5,"水平垂直运转速度","0-255 "]
[null,6,"调光","0-255"]
[null,7,"频闪","0-255"]
[null,8,"红色调光","0-255"]
[null,9,"绿色调光","0-255"]
[null,10,"蓝色调光","0-255"]
[null,11,"白色调光","0-255"]
[null,12,"颜色自走","0-255"]
[null,13,"电机自走","0-255"]
[null,14,"自走速度","0-255"]
[null,15,"复位","250-255（5秒）"]
[]
[null,"13通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"垂直运转","0-255"]
[null,3,"水平垂直运转速度","0-255 "]
[null,4,"调光","0-255"]
[null,5,"频闪","0-255"]
[null,6,"红色调光","0-255"]
[null,7,"绿色调光","0-255"]
[null,8,"蓝色调光","0-255"]
[null,9,"白色调光","0-255"]
[null,10,"颜色自走","0-255"]
[null,11,"电机自走","0-255"]
[null,12,"自走速度","0-255"]
[null,13,"复位","250-255（5秒）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}