{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":75,"n_cols":4,"rows_kept":75,"merged":[[0,1,0,3],[45,1,48,1],[50,1,53,1]],"flags":["formulas_cached_only"]}
[null,"六色调焦说明书"]
[]
[null,"DMXSet \nAddress","001-512","512地址设置"]
[]
[null,"Channel SET",12,"12通道设置"]
[null,null,19,"19通道设置"]
[]
[null,"Show Mode","Dmx Mode","控台模式"]
[null,null,"Fast Mode","快速运行模式"]
[null,null,"Slow Mode","慢速运行模式"]
[null,null,"Soud Mode","声控运行模式"]
[]
[null,"Sound Sense","0-99","声控灵敏度体调节"]
[]
[null,"Pan Inverse","OFF","X电机正转"]
[null,null,"ON","X电机反转"]
[]
[null,"Tite Inverse","OFF","Y电机正转"]
[null,null,"ON","Y电机反转"]
[]
[null,"While  balance","Red     0-255","红色调节"]
[null,null,"Green   0-255","绿色调节"]
[null,null,"Blue    0-255","蓝色调节"]
[null,null,"While   0-255 ","白色调节"]
[null,null,"Yellow  0-255","黄色调节"]
[null,null,"Purple  0-255","紫色调节"]
[]
[null,"Defaults \nConfimrm?","YES","初始化出厂"]
[]
[null,"Fixture \nREST","YES","系统复位"]
[]
[null,"19通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255 向上调节正转，向下调节反转"]
[null,2,"垂直运转","0-255 向上调节正转，向下调节反转"]
[null,3,"总调光","0-255 亮度整体调节"]
[null,4,"R调光","0-255 红色亮度调节"]
[null,5,"G调光","0-255 绿色亮度调节"]
[null,6,"B调光","0-255 蓝色亮度调节"]
[null,7,"W调光","0-255 白色亮度调节"]
[null,8,"Y调光","0-255 黄色亮度调节"]
[null,9,"P调光","0-255 紫色亮度调节"]
[null,10,"频闪","0-255频闪调节，由慢到快"]
[null,11,"电机运行速度","0-255 水平，垂直电机运行速度"]
[null,12,"调焦电机","0-255"]
[null,13,"11-127","颜色组合变化"]
[null,null,"128-160","颜色跳变"]
[null,null,"161-200","颜色渐变1"]
[null,null,"201-255","颜色渐变2"]
[null,14,"速度调节","第13通道速度调节功能"]
[null,15,"0-10","其他通道作用"]
[null,null,"11-120","自走效果1"]
[null,null,"121-243","自走效果2"]
[null,null,"245-255","声控"]
[null,16,"内置效果速度","内置效果速度调节"]
[null,17,"水平运转微调","0-255 向上调节正转，向下调节反转"]
[null,18,"垂直运转微调","0-255 向上调节正转，向下调节反转"]
[null,19,"复位","150-200  复位"]
[]
[]
[]
[null,"12通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255 向上调节正转，向下调节反转"]
[null,2,"垂直运转","0-255 向上调节正转，向下调节反转"]
[null,3,"总调光","0-255 亮度整体调节"]
[null,4,"R调光","0-255 红色亮度调节"]
[null,5,"G调光","0-255 绿色亮度调节"]
[null,6,"B调光","0-255 蓝色亮度调节"]
[null,7,"W调光","0-255 白色亮度调节"]
[null,8,"Y调光","0-255 黄色亮度调节"]
[null,9,"P调光","0-255 紫色亮度调节"]
[null,10,"频闪","0-255频闪调节，由慢到快"]
[null,11,"电机运行速度","0-255 水平，垂直电机运行速度"]
[null,12,"调焦电机","0-255"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}