{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":103,"n_cols":4,"rows_kept":103,"merged":[[0,1,0,3],[53,1,57,1],[60,1,71,1],[72,1,80,1],[95,1,99,1]],"flags":["formulas_cached_only"]}
[null,"说明书"]
[null,"Addr","A001-A512","512地址设置"]
[]
[null,"CHnd","18CH","18通道设置"]
[null,null,"13CH","13通道设置"]
[]
[null,"SLnd","Auto","主机自走模式"]
[null,null,"Soun","主机声控模式"]
[null,null,"SL 1","控台模式"]
[null,null,"SL 2","副机模式"]
[]
[null,"SHnd","SH 0","效果0（推荐）"]
[null,null,"SH 1","效果1"]
[null,null,"SH 2","效果2"]
[null,null,"SH 3","效果3"]
[]
[]
[null,"SEnS","0-99","声控灵敏度体调节"]
[]
[null,"bLAnd","bLAc","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Soun","无512信号声控"]
[null,null,"HoLd","无512信号保持上次控台状态"]
[]
[null,"LEd","OFF","5秒后灭屏"]
[null,null,"ON","屏幕一直开启"]
[]
[null,"dISP","no","显示反向"]
[null,null,"YES","显示正向"]
[]
[null,"rPAN","no","X电机正转"]
[null,null,"YES","X电机反转"]
[]
[null,"rTiL","no","Y电机正转"]
[null,null,"YES","Y电机反转"]
[]
[null,"REST","YES","系统复位"]
[]
[]
[]
[null,"18通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"水平运转微调","0-255"]
[null,3,"垂直运转","0-255"]
[null,4,"垂直运转微调","0-255"]
[null,5,"水平垂直运转速度","0-255 "]
[null,6,"总调光","0-255"]
[null,7,"红色1总调光","0-255"]
[null,8,"绿色1总调光","0-255"]
[null,9,"蓝色1总调光","0-255"]
[null,10,"白色1总调光","0-255"]
[null,11,"颜色频闪","0-255"]
[null,12,"激光选择 "]
[null,null,"0-10","都灭 "]
[null,null,"11-100","红色激光"]
[null,null,"101-200","绿色激光"]
[null,null,"201-255","红色激光+绿色激光"]
[null,13,"激光频闪","0-255"]
[null,14,"激光图案","0-255"]
[null,15,"其他通道作用",0]
[null,null,"渐变","1-7"]
[null,null,"灯泡自走0","7-39"]
[null,null,"灯泡自走1","40-72"]
[null,null,"灯泡自走2","73-105"]
[null,null,"灯泡自走3","106-138"]
[null,null,"灯泡自走4","139-140"]
[null,null,"灯泡声控0","141-167"]
[null,null,"灯泡声控1","168-195"]
[null,null,"灯泡声控2","196-223"]
[null,null,"灯泡声控3","224-251"]
[null,null,"灯泡声控4","252-255"]
[null,16,"其他通道作用","0-15"]
[null,null,"自走3","16-44"]
[null,null,"自走2","45-74"]
[null,null,"自走1","75-104"]
[null,null,"自走0","105-128"]
[null,null,"声控3","129-157"]
[null,null,"声控2","158-187"]
[null,null,"声控1","188-217"]
[null,null,"声控0","218-255"]
[null,17,"自走速度/灵敏度","0-255"]
[null,18,"复位","250-255（5秒）"]
[]
[null,"13通道模式"]
[null,"通道","功能","说明"]
[null,1,"水平运转","0-255"]
[null,2,"垂直运转","0-255"]
[null,3,"水平垂直运转速度","0-255 "]
[null,4,"总调光","0-255"]
[null,5,"红色1总调光","0-255"]
[null,6,"绿色1总调光","0-255"]
[null,7,"蓝色1总调光","0-255"]
[null,8,"白色1总调光","0-255"]
[null,9,"颜色频闪","0-255"]
[null,10,"激光选择 "]
[null,null,"0-10","都灭 "]
[null,null,"11-100","红色激光"]
[null,null,"101-200","绿色激光"]
[null,null,"201-255","红色激光+绿色激光"]
[null,11,"激光频闪","0-255"]
[null,12,"激光图案","0-255"]
[null,13,"复位","250-255（5秒）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}