{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":183,"n_cols":5,"rows_kept":183,"merged":[[0,1,0,3],[39,1,40,1],[41,1,42,1],[63,1,64,1],[65,1,66,1],[112,1,113,1],[182,4,183,4]],"flags":["formulas_cached_only"]}
[null,"说明书"]
[null," Addre","001-512","512地址设置"]
[]
[null,"Chnd","07CH","7通道设置"]
[null,null,"10CH","10通道设置"]
[null,null,"16CH","16通道设置"]
[null,"Slnd       ","Auto","自动模式"]
[null,null,"Soun","声控模式"]
[null,null,"Slve 1","控台模式"]
[null,null,"Slve 2","副机模式"]
[null,"Shnd","Sh 0-9","效果0-效果9"]
[null,"Auto     Speed","0-100","自走速度调节"]
[null,"Sound     Sense","0-100","声控灵敏度调节"]
[null,"Nodmx      Set","Blac","无512信号归零"]
[null,null,"Auto","无512信号自走"]
[null,null,"Sound","无512信号声控"]
[null,"LED","OFF","开启灭屏"]
[null,null,"ON","关闭灭屏"]
[null,"Disp","Yes","关闭倒显示"]
[null,null,"ON","开启倒显示"]
[null,"RPan  ","OFF","X电机正转"]
[null,null,"ON","X电机反转"]
[null,"Rest","YES","系统复位"]
[]
[]
[null,"16 通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","X电机速度"]
[null,3,"0-255","0-255 亮度整体调节"]
[null,4,"0-255","BAR1   亮度调节"]
[null,5,"0-255","BAR2   亮度调节"]
[null,6,"0-255","BAR3   亮度调节"]
[null,7,"0-255","BAR4   亮度调节"]
[null,8,"0-255","BAR5   亮度调节"]
[null,9,"0-255","BAR6   亮度调节"]
[null,10,"0-255","BAR7   亮度调节"]
[null,11,"0-255","BAR8   亮度调节"]
[null,12,"0-255","频闪速度调节"]
[null,13,"0-127","LED 自走内置效果（0-9）"]
[null,null,"128-255","LED 声控内置效果（0-9）"]
[null,14,"0-127","自走内置效果（0-9）"]
[null,null,"128-255","声控内置效果（0-9）"]
[null,15,"0-255","速度/声控灵敏度"]
[null,16,"250-255","复位"]
[]
[null,"10 通道模式"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","X电机速度"]
[null,3,"0-255","BAR1   亮度调节"]
[null,4,"0-255","BAR2   亮度调节"]
[null,5,"0-255","BAR3   亮度调节"]
[null,6,"0-255","BAR4   亮度调节"]
[null,7,"0-255","BAR5   亮度调节"]
[null,8,"0-255","BAR6   亮度调节"]
[null,9,"0-255","BAR7   亮度调节"]
[null,10,"0-255","BAR8   亮度调节"]
[]
[null,"7 通道模式"]
[null,"通道","功能","说明"]
[null,1,"0-255","X电机运转"]
[null,2,"0-255","X电机速度"]
[null,3,"0-255","0-255 亮度整体调节"]
[null,4,"0-127","LED 自走内置效果（0-9）"]
[null,null,"128-255","LED 声控内置效果（0-9）"]
[null,5,"0-127","自走内置效果（0-9）"]
[null,null,"128-255","声控内置效果（0-9）"]
[null,6,"0-255","速度/声控灵敏度"]
[null,7,"250-255","复位"]
{"$rows_empty":43}
[null,"注意，此功能对无极旋转无效。无极旋转的时候要可以调整X轴的角度"]
{"$rows_empty":69}
[{"$nulls":4},"注意，此功能对无极旋转无效。无极旋转的时候要可以调整X轴的角度"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}